{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"macros":1,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":71,"n_cols":16,"rows_kept":71,"merged":[[0,0,0,15],[1,0,1,15],[2,6,2,15]],"flags":["formulas_cached_only"]}
["Table-1 ST: SCHEDULED TRIBE FEMALE HEADED HOUSEHOLDS BY PREDOMINANT MATERIALS OF ROOF AND WALL OF CENSUS HOUSES OCCUPIED BY THEM\n"]
["(Excluding Institutional Households)"]
[{"$nulls":6},"MATERIAL OF ROOF"]
["Table Name","State Code","District Code","Area Name","Total/\nRural/\nUrban","Material of wall","Total Number of female headed households","Grass/thatch/ bamboo/ wood/mud etc.","Plastic/ Polythene","Hand made tiles","Machine made tiles","Burnt brick","Stone/ Slate","G.I./metal/asbestos sheets","Concrete","Any other"]
[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16]
["HH4900T","31","000","STATE - LAKSHADWEEP","Total","All Material",{"v":4214,"d":"4,214"},58,1,16,{"v":1850,"d":"1,850"},4,18,302,{"v":1961,"d":"1,961"},4]
["HH4900T","31","000","STATE - LAKSHADWEEP","Total","Grass/thatch/bamboo etc.",50,30,0,0,14,0,0,6,0,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Total","Plastic/ Polythene",1,0,1,0,0,0,0,0,0,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Total","Mud/unburnt brick",9,0,0,0,5,0,0,1,3,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Total","Wood",1,0,0,0,1,0,0,0,0,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Total","Stone not packed with mortar",478,17,0,1,250,0,4,63,141,2]
["HH4900T","31","000","STATE - LAKSHADWEEP","Total","Stone packed with mortar",{"v":2180,"d":"2,180"},5,0,12,990,3,13,146,{"v":1010,"d":"1,010"},1]
["HH4900T","31","000","STATE - LAKSHADWEEP","Total","G.I./ metal/asbestos sheets",2,0,0,0,0,0,0,2,0,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Total","Burnt brick",{"v":1438,"d":"1,438"},6,0,3,588,1,1,79,759,1]
["HH4900T","31","000","STATE - LAKSHADWEEP","Total","Concrete",54,0,0,0,2,0,0,4,48,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Total","Any other",1,0,0,0,0,0,0,1,0,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Rural","All Material",732,25,1,0,464,1,2,48,188,3]
["HH4900T","31","000","STATE - LAKSHADWEEP","Rural","Grass/thatch/bamboo etc.",18,10,0,0,5,0,0,3,0,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Rural","Plastic/ Polythene",1,0,1,0,0,0,0,0,0,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Rural","Mud/unburnt brick",5,0,0,0,4,0,0,1,0,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Rural","Wood",0,0,0,0,0,0,0,0,0,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Rural","Stone not packed with mortar",161,10,0,0,115,0,0,9,25,2]
["HH4900T","31","000","STATE - LAKSHADWEEP","Rural","Stone packed with mortar",354,1,0,0,232,1,2,24,93,1]
["HH4900T","31","000","STATE - LAKSHADWEEP","Rural","G.I./ metal/asbestos sheets",0,0,0,0,0,0,0,0,0,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Rural","Burnt brick",192,4,0,0,108,0,0,11,69,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Rural","Concrete",1,0,0,0,0,0,0,0,1,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Rural","Any other",0,0,0,0,0,0,0,0,0,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Urban","All Material",{"v":3482,"d":"3,482"},33,0,16,{"v":1386,"d":"1,386"},3,16,254,{"v":1773,"d":"1,773"},1]
["HH4900T","31","000","STATE - LAKSHADWEEP","Urban","Grass/thatch/bamboo etc.",32,20,0,0,9,0,0,3,0,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Urban","Plastic/ Polythene",0,0,0,0,0,0,0,0,0,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Urban","Mud/unburnt brick",4,0,0,0,1,0,0,0,3,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Urban","Wood",1,0,0,0,1,0,0,0,0,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Urban","Stone not packed with mortar",317,7,0,1,135,0,4,54,116,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Urban","Stone packed with mortar",{"v":1826,"d":"1,826"},4,0,12,758,2,11,122,917,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Urban","G.I./ metal/asbestos sheets",2,0,0,0,0,0,0,2,0,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Urban","Burnt brick",{"v":1246,"d":"1,246"},2,0,3,480,1,1,68,690,1]
["HH4900T","31","000","STATE - LAKSHADWEEP","Urban","Concrete",53,0,0,0,2,0,0,4,47,0]
["HH4900T","31","000","STATE - LAKSHADWEEP","Urban","Any other",1,0,0,0,0,0,0,1,0,0]
["HH4900T","31","587","District - Lakshadweep","Total","All Material",{"v":4214,"d":"4,214"},58,1,16,{"v":1850,"d":"1,850"},4,18,302,{"v":1961,"d":"1,961"},4]
["HH4900T","31","587","District - Lakshadweep","Total","Grass/thatch/bamboo etc.",50,30,0,0,14,0,0,6,0,0]
["HH4900T","31","587","District - Lakshadweep","Total","Plastic/ Polythene",1,0,1,0,0,0,0,0,0,0]
["HH4900T","31","587","District - Lakshadweep","Total","Mud/unburnt brick",9,0,0,0,5,0,0,1,3,0]
["HH4900T","31","587","District - Lakshadweep","Total","Wood",1,0,0,0,1,0,0,0,0,0]
["HH4900T","31","587","District - Lakshadweep","Total","Stone not packed with mortar",478,17,0,1,250,0,4,63,141,2]
["HH4900T","31","587","District - Lakshadweep","Total","Stone packed with mortar",{"v":2180,"d":"2,180"},5,0,12,990,3,13,146,{"v":1010,"d":"1,010"},1]
["HH4900T","31","587","District - Lakshadweep","Total","G.I./ metal/asbestos sheets",2,0,0,0,0,0,0,2,0,0]
["HH4900T","31","587","District - Lakshadweep","Total","Burnt brick",{"v":1438,"d":"1,438"},6,0,3,588,1,1,79,759,1]
["HH4900T","31","587","District - Lakshadweep","Total","Concrete",54,0,0,0,2,0,0,4,48,0]
["HH4900T","31","587","District - Lakshadweep","Total","Any other",1,0,0,0,0,0,0,1,0,0]
["HH4900T","31","587","District - Lakshadweep","Rural","All Material",732,25,1,0,464,1,2,48,188,3]
["HH4900T","31","587","District - Lakshadweep","Rural","Grass/thatch/bamboo etc.",18,10,0,0,5,0,0,3,0,0]
["HH4900T","31","587","District - Lakshadweep","Rural","Plastic/ Polythene",1,0,1,0,0,0,0,0,0,0]
["HH4900T","31","587","District - Lakshadweep","Rural","Mud/unburnt brick",5,0,0,0,4,0,0,1,0,0]
["HH4900T","31","587","District - Lakshadweep","Rural","Wood",0,0,0,0,0,0,0,0,0,0]
["HH4900T","31","587","District - Lakshadweep","Rural","Stone not packed with mortar",161,10,0,0,115,0,0,9,25,2]
["HH4900T","31","587","District - Lakshadweep","Rural","Stone packed with mortar",354,1,0,0,232,1,2,24,93,1]
["HH4900T","31","587","District - Lakshadweep","Rural","G.I./ metal/asbestos sheets",0,0,0,0,0,0,0,0,0,0]
["HH4900T","31","587","District - Lakshadweep","Rural","Burnt brick",192,4,0,0,108,0,0,11,69,0]
["HH4900T","31","587","District - Lakshadweep","Rural","Concrete",1,0,0,0,0,0,0,0,1,0]
["HH4900T","31","587","District - Lakshadweep","Rural","Any other",0,0,0,0,0,0,0,0,0,0]
["HH4900T","31","587","District - Lakshadweep","Urban","All Material",{"v":3482,"d":"3,482"},33,0,16,{"v":1386,"d":"1,386"},3,16,254,{"v":1773,"d":"1,773"},1]
["HH4900T","31","587","District - Lakshadweep","Urban","Grass/thatch/bamboo etc.",32,20,0,0,9,0,0,3,0,0]
["HH4900T","31","587","District - Lakshadweep","Urban","Plastic/ Polythene",0,0,0,0,0,0,0,0,0,0]
["HH4900T","31","587","District - Lakshadweep","Urban","Mud/unburnt brick",4,0,0,0,1,0,0,0,3,0]
["HH4900T","31","587","District - Lakshadweep","Urban","Wood",1,0,0,0,1,0,0,0,0,0]
["HH4900T","31","587","District - Lakshadweep","Urban","Stone not packed with mortar",317,7,0,1,135,0,4,54,116,0]
["HH4900T","31","587","District - Lakshadweep","Urban","Stone packed with mortar",{"v":1826,"d":"1,826"},4,0,12,758,2,11,122,917,0]
["HH4900T","31","587","District - Lakshadweep","Urban","G.I./ metal/asbestos sheets",2,0,0,0,0,0,0,2,0,0]
["HH4900T","31","587","District - Lakshadweep","Urban","Burnt brick",{"v":1246,"d":"1,246"},2,0,3,480,1,1,68,690,1]
["HH4900T","31","587","District - Lakshadweep","Urban","Concrete",53,0,0,0,2,0,0,4,47,0]
["HH4900T","31","587","District - Lakshadweep","Urban","Any other",1,0,0,0,0,0,0,1,0,0]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}